RTL schematic

